# PLaSK User Manual

#### Page Contents

- EffectiveFrequencyCyl.Mode Class
  - `EffectiveFrequencyCyl.Mode`
  - Attributes
  - Descriptions
    - Attribute Details
      - `EffectiveFrequencyCyl.Mode.gain_integral`
      - `EffectiveFrequencyCyl.Mode.lam`
      - `EffectiveFrequencyCyl.Mode.loss`
      - `EffectiveFrequencyCyl.Mode.m`
      - `EffectiveFrequencyCyl.Mode.power`
      - `EffectiveFrequencyCyl.Mode.total_absorption`
      - `EffectiveFrequencyCyl.Mode.wavelength`

# EffectiveFrequencyCyl.Mode Class

class EffectiveFrequencyCyl.Mode

  Detailed information about the mode.

## Attributes

`gain_integral` | Total gain for the mode (mW).
`lam` | Alias for `wavelength`.
`loss` | Mode losses (1/cm).
`m` | LP_mn mode parameter describing angular dependence.
`power` | Total power emitted into the mode.
`total_absorption` | Cumulated absorption for the mode (mW).
`wavelength` | Mode wavelength (nm).

## Descriptions

### Attribute Details

EffectiveFrequencyCyl.Mode.gain_integral = <property object>

  Total gain for the mode (mW).

EffectiveFrequencyCyl.Mode.lam = <property object>

  Alias for `wavelength`.

EffectiveFrequencyCyl.Mode.loss = <property object>

  Mode losses (1/cm).

EffectiveFrequencyCyl.Mode.m = <property object>

  LP_mn mode parameter describing angular dependence.

EffectiveFrequencyCyl.Mode.power = <property object>

  Total power emitted into the mode.

EffectiveFrequencyCyl.Mode.total_absorption = <property object>

  Cumulated absorption for the mode (mW).

  This property combines gain in active region and absorption in the whole structure.

EffectiveFrequencyCyl.Mode.wavelength = <property object>

  Mode wavelength (nm).